zencontrol Control4 Driver Installation & Commissioning
==========================================================

To install these drivers:

0. Ensure your zencontrol controllers have the "Control4" and "TPI Advanced" paid features purchased and enabled. The controllers
   must also be on the same network as the Control4 Director.

   For more information see: https://support.zencontrol.com/hc/en-us/articles/360000134036-How-do-I-purchase-control-system-upgrades

1. Open Composer.

    IMPORTANT: Load each driver into the the Director manually by going to Driver > Add or Update Driver.

    This step is done manually because it uploads a copy of the driver onto the Control4 Director, which allows us to
    automatically commission the rest of the system.

2. In System Design > Items (right hand side) > Discovered tab - double click a controller to add it to your project.
3. Sync should begin as soon as the driver is added. Wait for sync to complete. This may take several minutes on a larger project,
   and longer if the controller has not yet finished its startup sequence (which involves scanning the DALI line).
4. After Sync as completed go to Actions > Commission with zencontrol to start the commissioning process.
   If composer freezes during commissioning (which can happen on large projects) this is OK. Just wait. The Control4 director is
   still running commissioning even though composer is unresponsive.
5. Review the commissioned drivers. You can convert ECG/zc_light_driver.c4z drivers to specific types (relay, fan and blind) by
    using the conversion options in the driver Actions tab.

DO NOT ATTEMPT TO MANUALLY ADD ZENCONTROL DRIVERS TO A PROJECT! They must all be created via Sync+Commission steps explained above.